If you use USB Dongles, for example for pCon.basket, pCon.dataclient, pCon.creator or pCon.xcad, you must stop the HASP LM service and Hardlock service befor installing the driver. Open the Aladdin monitor as Adminstrator. Go to Services -> Hardlock -> Stop Harlock and Service -> HASP -> Stop HASP LM Service. After the driver update you have to restart the services.

Alternativelly you can install the driver with following parameters:
haspdinst_9.XX_no_provisional_LDK.exe -i -ld -fi -fss -kp

Please Note: You need the -ld parameter for support the Legacy Drivers (Hardlock Dongles)